# MRT_Sync

MRT_Sync CameraID, TargetImgB, TargetImgC, TargetImgD

## Description

Syncs the specified camera while rendering to (up to) 3 additional target images. The first target image is specified using Set Camera To Image.
Note: All targets within a MRT render must share the same dimensions.

## Parameters

CameraID | INTEGER | ID of the camera which is to be rendered
TargetImgB | INTEGER | ImageID of the camera's second render target
TargetImgC | INTEGER | ImageID of the camera's third render target; Specify a value of 0 if less than 3 targets are needed
TargetImgD | INTEGER | ImageID of the camera's fourth render target; Specify a value of 0 if less than 4 targets are needed

MRT Commands
jGfx Command Index
jGfx Main